{"text_format":"2","workbook":"xls","n_sheets":6,"sheets":["Tabelle1","Tabelle2","Tabelle3","Tabelle4","Tabelle5","Tabelle6"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":61,"n_cols":7,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[null,"Bauvorhaben","…………………………………………………………………………","Muster-Ausschreibung Serge Ferrari AG, CH-8193 Eglisau"]
[null,null,null,"Fassade"]
[null,null,null,"Stamisol® FI"]
[]
[]
[null,"Position","Beschreibung der Arbeit:","Menge:","ME:","Preis:","Betrag:"]
[]
[]
[null,"01","Fassadenbahn Stamisol FI 2TAPE / Breite 250 cm"]
[null,null,"Material: Polyacrylat-Beschichtung auf Polyestervlies"]
[null,null,"Diffusionsoffen: sD-Wert ~ 0.05 m "]
[null,null,"Freibewitterungszeit: UV beständig, Einkleidung innerhalb von 4 Wochen"]
[null,null,"sehr gutes Brandverhalten: Euroclass BS3D0"]
[null,null,"10 Jahre Garantie"]
[null,null,"Reiskraft: 220/200 N/5 cm"]
[null,null,"Farbe: anthrazit"]
[null,null,"2 integrierte Klebezonen 90 mm zum Verkleben der"]
[null,null,"Überlappung"]
[null,null,"Speziell geeignet als technische Membran für geschlossene"]
[null,null,"und leicht geöffnete Fassaden aus Metall, Holz, Stein."]
[null,null,"Fugenbreite 15mm, Öffnungsanteil 10%"]
[]
[null,null,"Hersteller: Serge Ferrari AG, CH-8193 Eglisau"]
[null,null,"Telefon: 0041 (0)44 868 26 26"]
[null,null,"Telefax: 0041 (0)44 868 27 27"]
[null,null,"e-mail: infoch@sergeferrari.com            www.stamisol.com"]
[]
[null,"02","Stamisol-FI liefern und nach Herstellervorschrift."]
[null,null,"fachgerecht verlegen auf:"]
[null,null,"Unterkonstruktion aus Holzrahmen / Holzwerkstoffplatten","……………..","m2","………………..","…………………"]
[null,null,"Unterkonstruktion auf Metall","……………..","m2","………………..","…………………"]
[]
[null,"03","Zuschläge für: (beinhaltet immer liefern und montieren)"]
[]
[null,"03.01","winddichte Verklebung der Ueberlappung mit 2TAPE","..................","m²",".....................","......................"]
[]
[]
[null,"03.02","Anschlüsse an Mauerwerk mit","..................","m",".....................","......................"]
[null,null,"Stamcoll N55 oder Stamcoll AS"]
[]
[null,"03.03","Anschlüsse an Fenster aus Holz, Kunstoff, Metall mit","..................","m",".....................","......................"]
[null,null,"Stamcoll N55 oder Stamcoll AS"]
[null,null,"Bitte beachten Sie das Merkblatt \"Primer für nicht saugende Untergründe\""]
[]
[null,"03.04","Anschlüsse auf Blechabweiser mit","..................","m",".....................","......................"]
[null,null,"Stamcoll N55 und Stamcoll AS"]
[]
[null,"03.05","Anschlüsse an Abluftrohre mit","..................","Stk.",".....................","......................"]
[null,null,"Stamisol-Dunstrohranschlussmanschette (Farbe Orange)"]
[null,null,"Verklebt mit Stamcoll N55 oder Stamcoll AS"]
[null,null,"Verdeckte Montage möglich wegen Farbdifferenz"]
[null,null,"Achtung: auf Grund des Farbunterschieds ist eventuell eine"]
[null,null,"verdeckte Montage erforderlich."]
[]
[null,"03.06","Stamcoll Tape 25lm Breite 80mm 3 Rollen im Karton"]
[]
[]
[]
[null,"Total","Fassade",null,null,null,"........................"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle4","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle5","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle6","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}